Hazard log and risk register
Template by Folvan, https://folvan.com   |   Version 1, October 2026
Built from the public EASA Easy Access Rules text. Check every item against the current rule text and your own approved procedures. Not legal advice.
How to use
1. One row per hazard. Describe the hazard (what could cause harm), then the outcome you worry about.
2. Rate likelihood (1 to 5) and severity (A to E) with today's controls. The risk and its tolerability appear by themselves, using the matrix on the Matrix sheet.
3. Add mitigation with an owner and a date, rate the risk again with the mitigation in place, and record who accepted the remaining risk.
4. Set a review date. Review the log when an occurrence, an audit or a change touches a hazard, and at least once a year.
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	Hazard
	Outcome
	Existing controls
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L / S / risk
	Additional mitigation
	Owner and due date
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Risk matrix (example, adapt to your operation)
	Likelihood / Severity
	A Catastrophic
	B Hazardous
	C Major
	D Minor
	E Negligible

	5 Frequent
	5A Intolerable
	5B Intolerable
	5C Intolerable
	5D Tolerable
	5E Tolerable

	4 Occasional
	4A Intolerable
	4B Intolerable
	4C Tolerable
	4D Tolerable
	4E Tolerable

	3 Remote
	3A Intolerable
	3B Tolerable
	3C Tolerable
	3D Tolerable
	3E Acceptable

	2 Improbable
	2A Tolerable
	2B Tolerable
	2C Tolerable
	2D Acceptable
	2E Acceptable

	1 Extremely improbable
	1A Tolerable
	1B Acceptable
	1C Acceptable
	1D Acceptable
	1E Acceptable


Severity
	A Catastrophic
	Aircraft destroyed; one or more deaths.

	B Hazardous
	Serious injury; major aircraft damage; a large reduction in safety margins.

	C Major
	A serious incident; injury; a significant reduction in safety margins.

	D Minor
	An incident; operating limitations; use of emergency procedures.

	E Negligible
	Little or no effect on safety.


Likelihood
	5 Frequent
	Likely to happen many times; has happened often in our operation.

	4 Occasional
	Likely to happen sometimes; has happened in our operation.

	3 Remote
	Unlikely but possible; has happened at least once in our operation or at similar ones.

	2 Improbable
	Very unlikely; not known to have happened at operators like us.

	1 Extremely improbable
	Almost inconceivable that it will happen.


What each level means
	Intolerable
	Stop or change the activity until the risk is reduced. Not accepted at any level.

	Tolerable
	Accept only with mitigation in place and a decision by the accountable manager. Review it.

	Acceptable
	Accept. The safety manager records it and keeps it under review.


Columns from the example risk register in GM3 ORO.GEN.200(a)(3). The matrix, the definitions and who may accept each level are Folvan's example, not a rule: adapt them to your operation and approved procedures.
Free to use and adapt. Template by Folvan, guide at https://folvan.com/resources/aviation-risk-assessment/




